

To enter Recovery mode:


* Use an Ethernet cable to connect the gateway to your computer. (Recovery mode is  
  not supported on USBnet.)
* Press “Reset” button over 20s. (Release the button when the Power LED flashes amber.)
* Launch your browser and enter the IP address and port number  
  http://192.168.13.31:9191., you will enter to Recovery mode as below:




* Choose Aleos firmware -> press Update



* Wait for firmware installing



* After a minute, the screen is as below, press Reboot



* Wait device is rebooted, select Software and Firmware, and upgrade Radio firmware again.